0. O2^™ and OCT ANE^™ R12000 CPU Upgrade Information

This flier pr ovides information about installing an R12000 CPU and any necessary softwar e in an O2 or OCT ANE system. This upgrade is applicable only to systems with an R10000 CPU alr eady installed.

Checking Your Shipment

Included in this shipment ar e the following items: • 6.5.x^1 Overlay CD • Wrist strap • Reversible scr ewdriver • R12000 CPU pr ocessor module • Upgrade label

1 “The Overlay version of IRIX 6.5 software that you received with this shipment. Overlay software is labeled “IRIX 6.5.x, “x” referring to the current numbered version of the software, for example 6.5.3. Base software is referred to as IRIX 6.5.

Document Number 007-3725-001

O2^™ and OCTANE^™ R12000 CPU Upgrade Information

Installing the Software

Make sur e you install the softwar e befor e installing the har dwar e. You must have IRIX 6.5 base softwar e installed to be able to install the Overlay IRIX 6.5.x softwar e. For this upgrade, use the IRIX Overlay CD that shipped with this R12000 CPU har dwar e.

Note: IRIX 6.5 base softwar e does not ship with the pr ocessor upgrade. Contact your local sales r epresentative to or der the base IRIX 6.5.

To check your workstation’s IRIX® version, fr om the T oolchest > Desktop, open a Unix shell.

At the pr ompt, enter

uname -aR

To install the softwar e, follow the instr uctions in the softwar e installation booklet that came with your CDs.

Installing the Har dware

For instr uctions on installing the R12000 pr ocessor, see your owner ’s guide.

• For O2 owners, see the O2 Workstation Owner ’s Guide, Chapter 5, “Or dering, Removing, and Installing Replacement Parts”. This information is also found in the online O2 Workstation Hardwar e Reference Guide.

• For OCTANE owners, see the OCTANE Workstation Owner ’s Guide, Chapter 2, “Installing and Removing the CPU and Memory”.

O2^™ and OCTANE^™ R12000 CPU Upgrade Information

Attaching the Upgrade Label

Attach the OCT ANE upgrade label to the system label on the back of the workstation. Attach the O2 upgrade label near the system label on the bottom of the workstation.

Troubleshooting

If your workstation does not boot after installing the CPU, r eread the CPU installation instr uctions. Check to make sur e the new CPU is corr ectly seated. If you mistakenly installed the new R12000 CPU befor e installing the softwar e follow these steps (r efer to your owner ’s guide for instr uctions):

1. Remove the new CPU module.

2. Reinstall the old CPU module.

3. Install the softwar e.

4. Remove the old CPU module.

5. Install the new CPU module.

If you need further help to tr oubleshoot the installation, see your owner ’s guide. If necessary , contact your local authorized service pr ovider .

©1999, Silicon Graphics, Inc. All rights reserved. Silicon Graphics and IRIX are registered trademarks and the Silicon Graphics logo, O2, and OCTANE are trademarks of Silicon Graphics, Inc. R10000 is a registered trademark and R12000 is a trademark of MIPS Technologies, Inc.UNIXisa registered trademarkinthe UnitedStates and othercountries, licensed exclusively through X/Open Company, Ltd.